|  |
| --- |
| 20 ft standard shipping container dimensions |

|  |  |
| --- | --- |
| **Container Reference Code:** | **22GP** |

|  |  |
| --- | --- |
| **Container Application:** | **The 20 ft standard shipping container is for general purpose cargo.** |
| **Container Dimensions:** | Width | Height | Length |
| **Door opening in feet** | 7' 8 ⅛" | 7' 6 ¼" |  |
| **Door opening in meters** | 2.34 m | 2.29 m |  |
| **Interior dimensions in feet** | 7' 8 ⅝" | 7' 6 ¼" | 19' 4 ¼" |
| **Interior dimensions in meters** | 2.34 m | 2.29 m | 5.9 m |
| **Container Weight** | Max Gross | Tare | Max Payload |
| **Weight in lbs** | 52,831 lbs | 4,914 lbs | 47,899 lbs |
| **Weight in kg** | 23,956 kg | 2,229 kg | 21,727 kg |
| **Container Volume** | In CFT | In CBM |  |
| **Load Capacity** | 1,172 CFT | 33.2 CBM |  |
| 40 ft standard shipping container dimensions |

|  |  |
| --- | --- |
| **Container Reference Code:** | **42GP** |

|  |  |
| --- | --- |
| **Container Application:** | **The 40 ft standard shipping container is for general purpose cargo.** |
| **Container Dimensions:** | Width | Height | Length |
| **Door opening in feet** | 7' 8 ⅛" | 7' 6 ¼" |  |
| **Door opening in meters** | 2.34 m | 2.29 m |  |
| **Interior dimensions in feet** | 7' 8 ⅝" | 7' 10 ¼" | 37' 11 ¼" |
| **Interior dimensions in meters** | 2.352 m | 2.395 m | 12.01 m |
| **Container Weight** | Max Gross | Tare | Max Payload |
| **Weight in lbs** | 67,199 lbs | 5,220 lbs | 59,039 lbs |
| **Weight in kg** | 30,481 kg | 3,701 kg | 26,780 kg |
| **Container Volume** | In CFT | In CBM |  |
| **Load Capacity** | 2,389.75 CFT | 67.67 CBM |  |
| 40 ft high cube standard shipping container dimensions |

|  |  |
| --- | --- |
| **Container Reference Code:** | **40HQ or 40HC** |

|  |  |
| --- | --- |
| **Container Application:** | **The 40 ft high cube shipping container is larger than the 40 ft standard shipping container.** |
| **Container Dimensions:** | Width | Height | Length |
| **Door opening in feet** | 7' 8 ⅛" | 8' 6 ¼" |  |
| **Door opening in meters** | 2.34 m | 2.56 m |  |
| **Interior dimensions in feet** | 7' 8 ⅝" | 8' 10 ⅛" | 39' 5 ⅝" |
| **Interior dimensions in meters** | 2.352 m | 2.69 m | 12.01 m |
| **Container Weight** | Max Gross | Tare | Max Payload |
| **Weight in lbs** | 67,196 lbs | 8,747 lbs | 58,448 lbs |
| **Weight in kg** | 30,480 kg | 3,968 kg | 26,512 kg |
| **Container Volume** | In CFT | In CBM |  |
| **Load Capacity** | 2,694 CFT | 76.3 CBM |  |
| 45 ft high cube standard shipping container dimensions |

|  |  |
| --- | --- |
| **Container Reference Code:** | **L5GO** |

|  |  |
| --- | --- |
| **Container Application:** | **The 45 ft high cube shipping container is for general purpose cargo.** |
| **Container Dimensions:** | Width | Height | Length |
| **Door opening in feet** | 7' 9½" | 8' 5 ¾" |  |
| **Door opening in meters** | 2.37 m | 2.58 m |  |
| **Interior dimensions in feet** | 7' 11" | 8' 10" | 44' 4 ¾" |
| **Interior dimensions in meters** | 2.41 m | 2.69 m | 13.53 m |
| **Container Weight** | Max Gross | Tare | Max Payload |
| **Weight in lbs** | 74,960 lbs | 10,910 lbs | 64,050 lbs |
| **Weight in kg** | 3,4000 kg | 4,950 kg | 29,050 kg |
| **Container Volume** | In CFT | In CBM |  |
| **Load Capacity** | 3,122 CFT | 88.4 CBM |  |

|  |
| --- |
| 20 ft ventilated shipping container dimensions |

|  |  |
| --- | --- |
| **Container Reference Code:** | **22VH** |

|  |  |
| --- | --- |
| **Container Application:** | **The 20 ft ventilated shipping container is for cargo that requires ventilation, typically used to transport green coffee beans or similar cargo.** |
| **Container Dimensions:** | Width | Height | Length |
| **Door opening in feet** | 7' 8 ⅛" | 7' 6 ¼" |  |
| **Door opening in meters** | 2.34 m | 2.29 m |  |
| **Interior dimensions in feet** | 7' 8 ⅝" | 7' 10 ¼" | 19' 4 ¼" |
| **Interior dimensions in meters** | 2.352 m | 2.395 m | 5.9 m |
| **Container Weight** | Max Gross | Tare | Max Payload |
| **Weight in lbs** | 52,897 lbs | 5,297 lbs | 47,899 lbs |
| **Weight in kg** | 32,500 kg | 2,394 kg | 21,727 kg |
| **Container Volume** | In CFT | In CBM |  |
| **Load Capacity** | 1,172 CFT | 33.2 CBM |  |

|  |
| --- |
| 20 ft refrigerated shipping container dimensions |

|  |  |
| --- | --- |
| **Container Reference Code:** | **22RT** |

|  |  |
| --- | --- |
| **Container Application:** | **The 20 ft refrigerated shipping container is for cargo that requires temperature control.** |
| **Container Dimensions:** | Width | Height | Length |
| **Door opening in feet** | 7' 8 ⅛" | 7' 6 ¼" |  |
| **Door opening in meters** | 2.34 m | 2.29 m |  |
| **Interior dimensions in feet** | 7'6" | 7' 4 ⅞" | 17' 11 ⅝" |
| **Interior dimensions in meters** | 2.28 m | 2.33 m | 5.45 m |
| **Container Weight** | Max Gross | Tare | Max Payload |
| **Weight in lbs** | 67,200 lbs | 6,970 lbs | 60,230 lbs |
| **Weight in kg** | 30,480 kg | 3,160 kg | 27,320 kg |

|  |
| --- |
| 40 ft refrigerated shipping container dimensions |

|  |  |
| --- | --- |
| **Container Reference Code:** | **42RT** |

|  |  |
| --- | --- |
| **Container Application:** | **The 40 ft refrigerated shipping container is for cargo that requires temperature control or perishable cargo.** |
| **Container Dimensions:** | Width | Height | Length |
| **Door opening in feet** | 7' 5 ⅜" | 6' 11 ⅞" |  |
| **Door opening in meters** | 2.26 m | 2.13 m |  |
| **Interior dimensions in feet** | 7'5 ⅜" | 7' 1 ⅞" | 37' 11 ¼" |
| **Interior dimensions in meters** | 2.26 m | 2.18 m | 11.48 m |
| **Container Weight** | Max Gross | Tare | Max Payload |
| **Weight in lbs** | 67,053 lbs | 10,778 lbs | 56,275 lbs |
| **Weight in kg** | 30,415 kg | 4,889 kg | 25,526 kg |
| **Container Volume** | In CFT | In CBM |  |
| **Load Capacity** | 2,039.7 CFT | 57.76 CBM |  |

|  |
| --- |
| 20 ft flat rack shipping container dimensions |

|  |  |
| --- | --- |
| **Container Reference Code:** | **22PC** |

|  |  |
| --- | --- |
| **Container Application:** | **The 20 ft flat rack shipping container is for unusually heavy loads, over-sized cargo, construction equipment, building supplies or heavy machinery.** |
| **Container Dimensions:** | Width | Height | Length |
| **Interior dimensions in feet** | 8' | 7' 3 ⅞" | 19' 9 ¾" |
| **Interior dimensions in meters** | 2.438 m | 2.233 m | 5.638 m |
| **Container Weight** | Max Gross | Tare | Max Payload |
| **Weight in lbs** | 99,200 lbs | 6,400 lbs | 92,800 lbs |
| **Weight in kg** | 45,000 kg | 2,900 kg | 42,100 kg |
| **Load Capacity** | 1,154.3 CFT | 32.7 CBM |  |

|  |
| --- |
| 40 ft flat rack shipping container dimensions |

|  |  |
| --- | --- |
| **Container Reference Code:** | **42PC** |

|  |  |
| --- | --- |
| **Container Application:** | **The 40 ft flat rack shipping container is for over-sized cargo, heavy machinery, construction equipment, or supplies.** |
| **Container Dimensions:** | Width | Height | Length |
| **Door opening in feet** | NA | NA |  |
| **Door opening in meters** | NA | NA |  |
| **Interior dimensions in feet** | 7' 4" | 7' 5 ⅓" | 39' 3 ⅞" |
| **Interior dimensions in meters** | 2.23 m | 2.27 m | 11.98 m |
| **Container Weight** | Max Gross | Tare | Max Payload |
| **Weight in lbs** | 98,326 lbs | 12,897 lbs | 85,429 lbs |
| **Weight in kg** | 44,600 kg | 5,850 kg | 38,750 kg |
| **Container Volume** | In CFT | In CBM |  |
| **Load Capacity** | 1,860 CFT | 52.7 CBM |  |

|  |
| --- |
| 20 ft open top shipping container dimensions |

|  |  |
| --- | --- |
| **Container Reference Code:** | **22U1** |

|  |  |
| --- | --- |
| **Container Application:** | **The 20 ft open top shipping container is for over-height cargo and top loading.** |
| **Container Dimensions:** | Width | Height | Length |
| **Door opening in feet** | 7' 8 ⅛" | 7' 6 ¼" |  |
| **Door opening in meters** | 2.34 m | 2.29 m |  |
| **Interior dimensions in feet** | 7' 8 ⅝" | 7' 10 ¼" | 19' 4 ¼" |
| **Interior dimensions in meters** | 2.352 m | 2.395 m | 5.9 m |
| **Container Weight** | Max Gross | Tare | Max Payload |
| **Weight in lbs** | 52,897 lbs | 5,297 lbs | 47,619 lbs |
| **Weight in kg** | 23,994 kg | 2,394 kg | 21,600 kg |
| **Container Volume** | In CFT | In CBM |  |
| **Load Capacity** | 1,172 CFT | 33.2 CBM |  |
| 40 ft open top shipping container dimensions |

|  |  |
| --- | --- |
| **Container Reference Code:** | **42OT** |

|  |  |
| --- | --- |
| **Container Application:** | **The 40 ft open top shipping container is for top loading for excessively long or high cargo.** |
| **Container Dimensions:** | Width | Height | Length |
| **Door opening in feet** | 7' 8 ⅛" | 7' 6 ¼" |  |
| **Door opening in meters** | 2.34 m | 2.29 m |  |
| **Interior dimensions in feet** | 7' 8 ⅝" | 7' 10 ¼" | 39' 5 ⅝" |
| **Interior dimensions in meters** | 2.352 m | 2.395 m | 12.01 m |
| **Container Weight** | Max Gross | Tare | Max Payload |
| **Weight in lbs** | 67,196 lbs | 8,487 lbs | 58,709 lbs |
| **Weight in kg** | 30,480 kg | 3,850 kg | 26,630 kg |
| **Container Volume** | In CFT | In CBM |  |
| **Load Capacity** | 2,389.75 CFT | 66.67 CBM |  |

|  |
| --- |
| 20 ft ISO tank shipping container dimensions |

|  |  |
| --- | --- |
| **Container Reference Code:** | **22TO** |

|  |  |
| --- | --- |
| **Container Application:** | **The 20 ft tank shipping container is for food stuffs, oils, and chemicals.** |
| **Container Dimensions:** | Width | Height | Length |
| **Exterior dimensions in feet** | 8' | 8' 6" | 20" |
| **Exterior dimensions in meters** | 2.43 m | 2.59 m | 6.09 m |
| **Container Volume** | In U.S. Gallons | In Liters |  |
| **Load Capacity** | 6,450 gl | 26,001 lt |  |